**Underground Storage Tank (UST) Cathodic Protection Impressed Current Inspection Log**

40 CFR 280.31.c

UST systems with impressed current cathodic protection systems must be inspected every 60 days to ensure the equipment is operating properly. (If equipment is equipped with green light on front panel, is the light on? If the equipment is equipped with meters, record the meter readings.)

A.A.C. R18-12-231(B)(1)

Facility Name: Facility ID Number:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Inspection Date | Is Green Light On? | | Meter Readings | | | Initials | If Green Light not on, Action Taken |
| Yes | No | Volts | Amps | Hours |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |

**\*NOTE:** All UST cathodic protection systems must be inspected within six months of installation and at least every three years thereafter. The results of the last two inspections are required for review and must be maintained at the facility.